# Adafruit MAX31865 ![Build Status](https://github.com/adafruit/Adafruit_MAX31865/workflows/Arduino%20Library%20CI/badge.svg)

This is the Adafruit MAX31856 Arduino Library 

<a href="https://www.adafruit.com/products/3328"><img src="assets/image.jpg" height="300"/></a>

Tested and works great with the Adafruit Thermocouple Breakout w/MAX31856
   * http://www.adafruit.com/products/3328

These sensors use SPI to communicate, 4 pins are required to  
interface

Adafruit invests time and resources providing this open source code, 
please support Adafruit and open-source hardware by purchasing 
products from Adafruit!

Written by Limor Fried/Ladyada  for Adafruit Industries.  
BSD license, check license.txt for more information
All text above must be included in any redistribution
