#!/usr/bin/env bash
#
# Build tests for DUE (Atmel SAM3X8E ARM Cortex-M3)
#

# exit on first failure
set -e

restore_configs
opt_set LCD_LANGUAGE bg
opt_set MOTHERBOARD BOARD_RAMPS4DUE_EFB
opt_set TEMP_SENSOR_0 -2
opt_set TEMP_SENSOR_BED 2
opt_set GRID_MAX_POINTS_X 16
opt_set FANMUX0_PIN 53
opt_enable S_CURVE_ACCELERATION EEPROM_SETTINGS GCODE_MACROS \
           PIDTEMPBED FIX_MOUNTED_PROBE Z_SAFE_HOMING CODEPENDENT_XY_HOMING \
           EEPROM_SETTINGS SDSUPPORT BINARY_FILE_TRANSFER \
           BLINKM PCA9632 RGB_LED RGB_LED_R_PIN RGB_LED_G_PIN RGB_LED_B_PIN LED_CONTROL_MENU \
           NEOPIXEL_LED CASE_LIGHT_ENABLE CASE_LIGHT_USE_NEOPIXEL CASE_LIGHT_MENU \
           NOZZLE_PARK_FEATURE ADVANCED_PAUSE_FEATURE FILAMENT_RUNOUT_DISTANCE_MM FILAMENT_RUNOUT_SENSOR \
           AUTO_BED_LEVELING_BILINEAR Z_MIN_PROBE_REPEATABILITY_TEST DEBUG_LEVELING_FEATURE \
           SKEW_CORRECTION SKEW_CORRECTION_FOR_Z SKEW_CORRECTION_GCODE CALIBRATION_GCODE \
           BACKLASH_COMPENSATION BACKLASH_GCODE BAUD_RATE_GCODE BEZIER_CURVE_SUPPORT \
           FWRETRACT ARC_SUPPORT ARC_P_CIRCLES CNC_WORKSPACE_PLANES CNC_COORDINATE_SYSTEMS \
           PSU_CONTROL AUTO_POWER_CONTROL \
           SLOW_PWM_HEATERS THERMAL_PROTECTION_CHAMBER \
           PINS_DEBUGGING MAX7219_DEBUG M114_DETAIL \
           EXTENSIBLE_UI
opt_add    EXTUI_EXAMPLE
opt_set E0_AUTO_FAN_PIN 8
opt_set EXTRUDER_AUTO_FAN_SPEED 100
opt_set TEMP_SENSOR_CHAMBER 3
opt_set HEATER_CHAMBER_PIN 45
exec_test $1 $2 "RAMPS4DUE_EFB with ABL (Bilinear), EXTENSIBLE_UI, S-Curve, many options."

restore_configs
opt_set MOTHERBOARD BOARD_RADDS
opt_enable USE_XMAX_PLUG USE_YMAX_PLUG ENDSTOPPULLUPS BLTOUCH AUTO_BED_LEVELING_BILINEAR \
           Z_MULTI_ENDSTOPS Z_STEPPER_AUTO_ALIGN Z_STEPPER_ALIGN_KNOWN_STEPPER_POSITIONS \
           Z_SAFE_HOMING
           #TOUCH_UI_FTDI_EVE LCD_ALEPHOBJECTS_CLCD_UI OTHER_PIN_LAYOUT
opt_set NUM_Z_STEPPER_DRIVERS 3
opt_add Z2_MAX_ENDSTOP_INVERTING false
opt_add Z3_MAX_ENDSTOP_INVERTING false
opt_add Z2_MAX_PIN 2
opt_add Z3_MAX_PIN 3
pins_set ramps/RAMPS X_MAX_PIN -1
pins_set ramps/RAMPS Y_MAX_PIN -1
exec_test $1 $2 "RADDS with ABL (Bilinear), Triple Z Axis, Z_STEPPER_AUTO_ALIGN"

#
# Test SWITCHING_EXTRUDER
#
restore_configs
opt_set LCD_LANGUAGE fi
opt_set MOTHERBOARD BOARD_RAMPS4DUE_EEF
opt_set EXTRUDERS 2
opt_set NUM_SERVOS 1
opt_enable SWITCHING_EXTRUDER ULTIMAKERCONTROLLER BEEP_ON_FEEDRATE_CHANGE POWER_LOSS_RECOVERY
exec_test $1 $2 "RAMPS4DUE_EEF with SWITCHING_EXTRUDER, POWER_LOSS_RECOVERY"
